## @file
#  Open Virtual Machine Firmware: FDF
#
#  Copyright (c) 2006 - 2017, Intel Corporation. All rights reserved.<BR>
#  (C) Copyright 2016 Hewlett Packard Enterprise Development LP<BR>
#
#  This program and the accompanying materials
#  are licensed and made available under the terms and conditions of the BSD License
#  which accompanies this distribution. The full text of the license may be found at
#  http://opensource.org/licenses/bsd-license.php
#
#  THE PROGRAM IS DISTRIBUTED UNDER THE BSD LICENSE ON AN "AS IS" BASIS,
#  WITHOUT WARRANTIES OR REPRESENTATIONS OF ANY KIND, EITHER EXPRESS OR IMPLIED.
#
##

################################################################################

[Defines]
!include OvmfPkg.fdf.inc

#
# Build the variable store and the firmware code as one unified flash device
# image.
#
[FD.OVMF]
BaseAddress   = $(FW_BASE_ADDRESS)
Size          = $(FW_SIZE)
ErasePolarity = 1
BlockSize     = $(BLOCK_SIZE)
NumBlocks     = $(FW_BLOCKS)

!include VarStore.fdf.inc

$(VARS_SIZE)|$(FVMAIN_SIZE)
FV = FVMAIN_COMPACT

$(SECFV_OFFSET)|$(SECFV_SIZE)
FV = SECFV

#
# Build the variable store and the firmware code as separate flash device
# images.
#
[FD.OVMF_VARS]
BaseAddress   = $(FW_BASE_ADDRESS)
Size          = $(VARS_SIZE)
ErasePolarity = 1
BlockSize     = $(BLOCK_SIZE)
NumBlocks     = $(VARS_BLOCKS)

!include VarStore.fdf.inc

[FD.OVMF_CODE]
BaseAddress   = $(CODE_BASE_ADDRESS)
Size          = $(CODE_SIZE)
ErasePolarity = 1
BlockSize     = $(BLOCK_SIZE)
NumBlocks     = $(CODE_BLOCKS)

0x00000000|$(FVMAIN_SIZE)
FV = FVMAIN_COMPACT

$(FVMAIN_SIZE)|$(SECFV_SIZE)
FV = SECFV

################################################################################

[FD.MEMFD]
BaseAddress   = $(MEMFD_BASE_ADDRESS)
Size          = 0xB00000
ErasePolarity = 1
BlockSize     = 0x10000
NumBlocks     = 0xB0

0x000000|0x006000
gUefiOvmfPkgTokenSpaceGuid.PcdOvmfSecPageTablesBase|gUefiOvmfPkgTokenSpaceGuid.PcdOvmfSecPageTablesSize

0x006000|0x001000
gUefiOvmfPkgTokenSpaceGuid.PcdOvmfLockBoxStorageBase|gUefiOvmfPkgTokenSpaceGuid.PcdOvmfLockBoxStorageSize

0x007000|0x001000
gEfiMdePkgTokenSpaceGuid.PcdGuidedExtractHandlerTableAddress|gUefiOvmfPkgTokenSpaceGuid.PcdGuidedExtractHandlerTableSize

0x010000|0x010000
gUefiOvmfPkgTokenSpaceGuid.PcdOvmfSecPeiTempRamBase|gUefiOvmfPkgTokenSpaceGuid.PcdOvmfSecPeiTempRamSize

0x020000|0x0E0000
gUefiOvmfPkgTokenSpaceGuid.PcdOvmfPeiMemFvBase|gUefiOvmfPkgTokenSpaceGuid.PcdOvmfPeiMemFvSize
FV = PEIFV

0x100000|0xA00000
gUefiOvmfPkgTokenSpaceGuid.PcdOvmfDxeMemFvBase|gUefiOvmfPkgTokenSpaceGuid.PcdOvmfDxeMemFvSize
FV = DXEFV

################################################################################

[FV.SECFV]
FvNameGuid         = 763BED0D-DE9F-48F5-81F1-3E90E1B1A015
BlockSize          = 0x1000
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

#
# SEC Phase modules
#
# The code in this FV handles the initial firmware startup, and
# decompresses the PEI and DXE FVs which handles the rest of the boot sequence.
#
INF  OvmfPkg/Sec/SecMain.inf

INF  RuleOverride=RESET_VECTOR OvmfPkg/ResetVector/ResetVector.inf

################################################################################
[FV.PEIFV]
FvNameGuid         = 6938079B-B503-4E3D-9D24-B28337A25806
BlockSize          = 0x10000
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

APRIORI PEI {
  INF  MdeModulePkg/Universal/PCD/Pei/Pcd.inf
}

#
#  PEI Phase modules
#
INF  MdeModulePkg/Core/Pei/PeiMain.inf
INF  MdeModulePkg/Universal/PCD/Pei/Pcd.inf
INF  MdeModulePkg/Universal/ReportStatusCodeRouter/Pei/ReportStatusCodeRouterPei.inf
INF  MdeModulePkg/Universal/StatusCodeHandler/Pei/StatusCodeHandlerPei.inf
INF  OvmfPkg/PlatformPei/PlatformPei.inf
INF  MdeModulePkg/Core/DxeIplPeim/DxeIpl.inf
INF  UefiCpuPkg/Universal/Acpi/S3Resume2Pei/S3Resume2Pei.inf
!if $(SMM_REQUIRE) == TRUE
INF  OvmfPkg/SmmAccess/SmmAccessPei.inf
!endif
INF  UefiCpuPkg/CpuMpPei/CpuMpPei.inf

################################################################################

[FV.DXEFV]
FvForceRebase      = FALSE
FvNameGuid         = 7CB8BDC9-F8EB-4F34-AAEA-3EE4AF6516A1
BlockSize          = 0x10000
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

APRIORI DXE {
  INF  MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
  INF  MdeModulePkg/Universal/PCD/Dxe/Pcd.inf
  INF  OvmfPkg/AmdSevDxe/AmdSevDxe.inf
!if $(SMM_REQUIRE) == FALSE
  INF  OvmfPkg/QemuFlashFvbServicesRuntimeDxe/FvbServicesRuntimeDxe.inf
!endif
}

#
# DXE Phase modules
#
INF  MdeModulePkg/Core/Dxe/DxeMain.inf

INF  MdeModulePkg/Universal/ReportStatusCodeRouter/RuntimeDxe/ReportStatusCodeRouterRuntimeDxe.inf
INF  MdeModulePkg/Universal/StatusCodeHandler/RuntimeDxe/StatusCodeHandlerRuntimeDxe.inf
INF  MdeModulePkg/Universal/PCD/Dxe/Pcd.inf

INF  MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
INF  MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
INF  MdeModulePkg/Universal/EbcDxe/EbcDxe.inf
INF  PcAtChipsetPkg/8259InterruptControllerDxe/8259.inf
INF  UefiCpuPkg/CpuIo2Dxe/CpuIo2Dxe.inf
INF  UefiCpuPkg/CpuDxe/CpuDxe.inf
INF  PcAtChipsetPkg/8254TimerDxe/8254Timer.inf
INF  OvmfPkg/IncompatiblePciDeviceSupportDxe/IncompatiblePciDeviceSupport.inf
INF  OvmfPkg/PciHotPlugInitDxe/PciHotPlugInit.inf
INF  MdeModulePkg/Bus/Pci/PciHostBridgeDxe/PciHostBridgeDxe.inf
INF  MdeModulePkg/Bus/Pci/PciBusDxe/PciBusDxe.inf
INF  MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
INF  MdeModulePkg/Universal/Metronome/Metronome.inf
INF  PcAtChipsetPkg/PcatRealTimeClockRuntimeDxe/PcatRealTimeClockRuntimeDxe.inf

INF  OvmfPkg/BlockMmioToBlockIoDxe/BlockIo.inf
INF  OvmfPkg/VirtioPciDeviceDxe/VirtioPciDeviceDxe.inf
INF  OvmfPkg/Virtio10Dxe/Virtio10.inf
INF  OvmfPkg/VirtioBlkDxe/VirtioBlk.inf
INF  OvmfPkg/VirtioScsiDxe/VirtioScsi.inf
INF  OvmfPkg/VirtioRngDxe/VirtioRng.inf
INF  OvmfPkg/XenIoPciDxe/XenIoPciDxe.inf
INF  OvmfPkg/XenBusDxe/XenBusDxe.inf
INF  OvmfPkg/XenPvBlkDxe/XenPvBlkDxe.inf

!if $(SECURE_BOOT_ENABLE) == TRUE
  INF  SecurityPkg/VariableAuthenticated/SecureBootConfigDxe/SecureBootConfigDxe.inf
!endif

INF  MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf
INF  MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
INF  MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
INF  MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
INF  MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
INF  MdeModulePkg/Universal/Console/GraphicsConsoleDxe/GraphicsConsoleDxe.inf
INF  MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
INF  MdeModulePkg/Universal/DriverHealthManagerDxe/DriverHealthManagerDxe.inf
INF  MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
INF  MdeModulePkg/Application/UiApp/UiApp.inf
INF  MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
INF  MdeModulePkg/Universal/PrintDxe/PrintDxe.inf
INF  MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
INF  MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
INF  MdeModulePkg/Universal/Disk/RamDiskDxe/RamDiskDxe.inf
INF  MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf
INF  MdeModulePkg/Bus/Scsi/ScsiBusDxe/ScsiBusDxe.inf
INF  MdeModulePkg/Bus/Scsi/ScsiDiskDxe/ScsiDiskDxe.inf
INF  OvmfPkg/SataControllerDxe/SataControllerDxe.inf
INF  MdeModulePkg/Bus/Ata/AtaAtapiPassThru/AtaAtapiPassThru.inf
INF  MdeModulePkg/Bus/Ata/AtaBusDxe/AtaBusDxe.inf
INF  MdeModulePkg/Bus/Pci/NvmExpressDxe/NvmExpressDxe.inf
INF  MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf
INF  MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
INF  MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
INF  MdeModulePkg/Universal/MemoryTest/NullMemoryTestDxe/NullMemoryTestDxe.inf

INF  PcAtChipsetPkg/IsaAcpiDxe/IsaAcpi.inf
INF  IntelFrameworkModulePkg/Bus/Isa/IsaBusDxe/IsaBusDxe.inf

!ifndef $(SOURCE_DEBUG_ENABLE)
INF  IntelFrameworkModulePkg/Bus/Isa/IsaSerialDxe/IsaSerialDxe.inf
!endif

INF  IntelFrameworkModulePkg/Bus/Isa/Ps2KeyboardDxe/Ps2keyboardDxe.inf
INF  IntelFrameworkModulePkg/Bus/Isa/IsaFloppyDxe/IsaFloppyDxe.inf

INF  MdeModulePkg/Universal/SmbiosDxe/SmbiosDxe.inf
INF  OvmfPkg/SmbiosPlatformDxe/SmbiosPlatformDxe.inf

INF  MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf
INF  OvmfPkg/AcpiPlatformDxe/AcpiPlatformDxe.inf
INF  RuleOverride=ACPITABLE OvmfPkg/AcpiTables/AcpiTables.inf
INF  MdeModulePkg/Universal/Acpi/S3SaveStateDxe/S3SaveStateDxe.inf
INF  MdeModulePkg/Universal/Acpi/BootScriptExecutorDxe/BootScriptExecutorDxe.inf
INF  MdeModulePkg/Universal/Acpi/BootGraphicsResourceTableDxe/BootGraphicsResourceTableDxe.inf

INF  FatPkg/EnhancedFatDxe/Fat.inf

!ifndef $(USE_OLD_SHELL)
INF  ShellPkg/DynamicCommand/TftpDynamicCommand/TftpDynamicCommand.inf
INF  ShellPkg/Application/Shell/Shell.inf
!else
INF  RuleOverride = BINARY EdkShellBinPkg/FullShell/FullShell.inf
!endif

INF MdeModulePkg/Logo/LogoDxe.inf

#
# Network modules
#
!if $(E1000_ENABLE)
  FILE DRIVER = 5D695E11-9B3F-4b83-B25F-4A8D5D69BE07 {
    SECTION PE32 = Intel3.5/EFIX64/E3522X2.EFI
  }
!endif
  INF  MdeModulePkg/Universal/Network/SnpDxe/SnpDxe.inf
  INF  MdeModulePkg/Universal/Network/DpcDxe/DpcDxe.inf
  INF  MdeModulePkg/Universal/Network/MnpDxe/MnpDxe.inf
  INF  MdeModulePkg/Universal/Network/VlanConfigDxe/VlanConfigDxe.inf
  INF  MdeModulePkg/Universal/Network/ArpDxe/ArpDxe.inf
  INF  MdeModulePkg/Universal/Network/Dhcp4Dxe/Dhcp4Dxe.inf
  INF  MdeModulePkg/Universal/Network/Ip4Dxe/Ip4Dxe.inf
  INF  MdeModulePkg/Universal/Network/Mtftp4Dxe/Mtftp4Dxe.inf
  INF  MdeModulePkg/Universal/Network/Udp4Dxe/Udp4Dxe.inf
!if $(NETWORK_IP6_ENABLE) == TRUE
  INF  NetworkPkg/Ip6Dxe/Ip6Dxe.inf
  INF  NetworkPkg/TcpDxe/TcpDxe.inf
  INF  NetworkPkg/Udp6Dxe/Udp6Dxe.inf
  INF  NetworkPkg/Dhcp6Dxe/Dhcp6Dxe.inf
  INF  NetworkPkg/Mtftp6Dxe/Mtftp6Dxe.inf
  INF  NetworkPkg/UefiPxeBcDxe/UefiPxeBcDxe.inf
  INF  NetworkPkg/IScsiDxe/IScsiDxe.inf
!else
  INF  MdeModulePkg/Universal/Network/Tcp4Dxe/Tcp4Dxe.inf
  INF  MdeModulePkg/Universal/Network/UefiPxeBcDxe/UefiPxeBcDxe.inf
  INF  MdeModulePkg/Universal/Network/IScsiDxe/IScsiDxe.inf
!endif
!if $(HTTP_BOOT_ENABLE) == TRUE
  INF  NetworkPkg/DnsDxe/DnsDxe.inf
  INF  NetworkPkg/HttpUtilitiesDxe/HttpUtilitiesDxe.inf
  INF  NetworkPkg/HttpDxe/HttpDxe.inf
  INF  NetworkPkg/HttpBootDxe/HttpBootDxe.inf
!endif
!if $(TLS_ENABLE) == TRUE
  INF  NetworkPkg/TlsDxe/TlsDxe.inf
  INF  NetworkPkg/TlsAuthConfigDxe/TlsAuthConfigDxe.inf
!endif
  INF  OvmfPkg/VirtioNetDxe/VirtioNet.inf

#
# Usb Support
#
INF  MdeModulePkg/Bus/Pci/UhciDxe/UhciDxe.inf
INF  MdeModulePkg/Bus/Pci/EhciDxe/EhciDxe.inf
INF  MdeModulePkg/Bus/Pci/XhciDxe/XhciDxe.inf
INF  MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf
INF  MdeModulePkg/Bus/Usb/UsbKbDxe/UsbKbDxe.inf
INF  MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf

!ifdef $(CSM_ENABLE)
INF  IntelFrameworkModulePkg/Csm/BiosThunk/VideoDxe/VideoDxe.inf
INF  IntelFrameworkModulePkg/Csm/LegacyBiosDxe/LegacyBiosDxe.inf
INF  RuleOverride=CSM OvmfPkg/Csm/Csm16/Csm16.inf
!endif

INF  OvmfPkg/QemuVideoDxe/QemuVideoDxe.inf
INF  OvmfPkg/VirtioGpuDxe/VirtioGpu.inf
INF  OvmfPkg/PlatformDxe/Platform.inf
INF  OvmfPkg/AmdSevDxe/AmdSevDxe.inf
INF  OvmfPkg/IoMmuDxe/IoMmuDxe.inf

!if $(SMM_REQUIRE) == TRUE
INF  OvmfPkg/SmmAccess/SmmAccess2Dxe.inf
INF  OvmfPkg/SmmControl2Dxe/SmmControl2Dxe.inf
INF  UefiCpuPkg/CpuS3DataDxe/CpuS3DataDxe.inf
INF  MdeModulePkg/Core/PiSmmCore/PiSmmIpl.inf
INF  MdeModulePkg/Core/PiSmmCore/PiSmmCore.inf
INF  SMMRootkit/SMMRootkit.inf
INF  UefiCpuPkg/CpuIo2Smm/CpuIo2Smm.inf
INF  MdeModulePkg/Universal/LockBox/SmmLockBox/SmmLockBox.inf
INF  UefiCpuPkg/PiSmmCpuDxeSmm/PiSmmCpuDxeSmm.inf

#
# Variable driver stack (SMM)
#
INF  OvmfPkg/QemuFlashFvbServicesRuntimeDxe/FvbServicesSmm.inf
INF  MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteSmm.inf
INF  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableSmm.inf
INF  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableSmmRuntimeDxe.inf

!else

#
# Variable driver stack (non-SMM)
#
INF  OvmfPkg/QemuFlashFvbServicesRuntimeDxe/FvbServicesRuntimeDxe.inf
INF  OvmfPkg/EmuVariableFvbRuntimeDxe/Fvb.inf
INF  MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
INF  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf
!endif

################################################################################

[FV.FVMAIN_COMPACT]
FvNameGuid         = 48DB5E17-707C-472D-91CD-1613E7EF51B0
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

FILE FV_IMAGE = 9E21FD93-9C72-4c15-8C4B-E77F1DB2D792 {
   SECTION GUIDED EE4E5898-3914-4259-9D6E-DC7BD79403CF PROCESSING_REQUIRED = TRUE {
     #
     # These firmware volumes will have files placed in them uncompressed,
     # and then both firmware volumes will be compressed in a single
     # compression operation in order to achieve better overall compression.
     #
     SECTION FV_IMAGE = PEIFV
     SECTION FV_IMAGE = DXEFV
   }
 }

!include DecomprScratchEnd.fdf.inc

################################################################################

[Rule.Common.SEC]
  FILE SEC = $(NAMED_GUID) {
    PE32     PE32           $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING ="$(MODULE_NAME)" Optional
    VERSION  STRING ="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.PEI_CORE]
  FILE PEI_CORE = $(NAMED_GUID) {
    PE32     PE32   Align=Auto    $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING ="$(MODULE_NAME)" Optional
    VERSION  STRING ="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.PEIM]
  FILE PEIM = $(NAMED_GUID) {
     PEI_DEPEX PEI_DEPEX Optional        $(INF_OUTPUT)/$(MODULE_NAME).depex
     PE32      PE32   Align=Auto         $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI       STRING="$(MODULE_NAME)" Optional
     VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_CORE]
  FILE DXE_CORE = $(NAMED_GUID) {
    PE32     PE32           $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX Optional      $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
    RAW ACPI  Optional               |.acpi
    RAW ASL   Optional               |.aml
  }

[Rule.Common.DXE_RUNTIME_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX Optional      $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX Optional      $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_DRIVER.BINARY]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional      |.depex
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_APPLICATION]
  FILE APPLICATION = $(NAMED_GUID) {
    PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_APPLICATION.BINARY]
  FILE APPLICATION = $(NAMED_GUID) {
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.USER_DEFINED.ACPITABLE]
  FILE FREEFORM = $(NAMED_GUID) {
    RAW ACPI               |.acpi
    RAW ASL                |.aml
  }

[Rule.Common.USER_DEFINED.CSM]
  FILE FREEFORM = $(NAMED_GUID) {
    RAW BIN                |.bin
  }

[Rule.Common.SEC.RESET_VECTOR]
  FILE RAW = $(NAMED_GUID) {
    RAW BIN   Align = 16   |.bin
  }

[Rule.Common.SMM_CORE]
  FILE SMM_CORE = $(NAMED_GUID) {
    PE32     PE32           $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_SMM_DRIVER]
  FILE SMM = $(NAMED_GUID) {
    SMM_DEPEX    SMM_DEPEX Optional      $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }
